LED recessed downlights, Cantone series. Four different covers in white, chrome, chrome matt and brushed metal, available in a round/square version. Operating unit can be dimmed (TRIAC/DALI dimmer), external. Version with CASAMBI® Bluetooth control available.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 8,1 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 450 lm

Colour temperature: 2700 K

Light source: LED

Physical data:

Length (L): 92 mm

Width (B): 92 mm

Height (H): 50 mm

Ceiling Cut-out ø: 68 mm

Manufacturer: RP-Technik GmbH