CASAMBI® motion detectors consist of integrated CASAMBI® technology and make it possible to control luminaires without wiring work. Use the CASAMBI® app to configure parameters such as brightness and automatically switching on and off at dusk or movement. This can result in savings of up to 90%. The sensors are available in various designs for ceiling mounting or recessed installation and various detection zones from 5 to 28 m.  
  
  
 Passive infrared sensor for recessed ceiling mounting  
 Detection zone: 5-7 m  
 Colour: white  
 IP20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 79 mm

Width (B): 85 mm

Height (H): 85 mm

Ceiling Cut-out ø: 60 mm

Manufacturer: RP-Technik GmbH