The CBU-TED-LR module is an elegant Bluetooth-controlled CASAMBI® phase-cut dimmer that allows for smooth dimming of all available light sources. It can be installed behind a conventional light switch, in a luminaire, or in a junction box. With the new Long Range feature, you can now enjoy reliable control from even greater distances.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Output max.: 100 W

Acceptance tests:

Physical data:

Manufacturer: RP-Technik GmbH