The CBU-TED module is a Bluetooth-controlled CASAMBI®trailing-edge dimmer that enables all available illuminants to be continuously dimmed. It can  
also be used to switch luminaires on and off, and can be installed behind a conventional light switch, in a luminaire or in a terminal box.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Output max.: 100 W

Switching output: 100 W

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 40,4 mm

Width (B): 36,3 mm

Height (H): 14 mm

Manufacturer: RP-Technik GmbH