LED recessed-mounted luminaire, AVE series. Round/square shape. Aluminium frame, white, powder-coated. Diffuser made from plastic (PMMA), opal. Power supply, can be switched or dimmed (DALI/TRIAC dimmer), internal. Version with CASAMBI® Bluetooth control available.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Impact resistance: IK 03

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 24 W

Photometrical data:

Rated luminous flux: 2.000 lm

Colour temperature: 4000 K

UGR: 25.9

Light source: LED

Physical data:

Height (H): 12 mm

Ceiling Cut-out ø: 285 mm

Diameter ø: 300 mm

Manufacturer: RP-Technik GmbH