LED ceiling- and wall-mounted luminaire, PORIO series, recessed design, as the basic lighting for commercial and residential rooms. Housing made from steel plate, white, powder-coated. Diffuser made from plastic (PMMA), opal, UV-stabilised. Operating unit can be switched or dimmed (DALI dimmer), integrated. Version with CASAMBI Bluetooth control available. DC compatible.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 33 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 3.000 lm

Colour temperature: 4000 K

UGR: 20.6

Light source: LED

Physical data:

Height (H): 90 mm

Diameter ø: 464 mm

Manufacturer: RP-Technik GmbH