LED ceiling- and wall-mounted luminaire, ZORRO. Housing made from steel plate, white, powder-coated. Diffuser made from plastic (PC), opal, UV-stabilised. Operating unit can be switched or dimmed (DALI dimmer), integrated. Version with CASAMBI® Bluetooth control available. DC compatible. NANO protection on request.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 40

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 44 W

Photometrical data:

Rated luminous flux: 5.000 lm

Colour temperature: 4000 K

UGR: 26.7

Light source: LED

Physical data:

Length (L): 1.100 mm

Width (B): 165 mm

Height (H): 63 mm

Manufacturer: RP-Technik GmbH