LED recessed downlight, BASE series. Can be swivelled in both directions. Housing made from steel plate, white, powder-coated.  Aluminium reflector with 2 beam angles (24° and 40°). Operating unit can be switched or dimmed (DALI dimmer), external. UGR