This module can be fitted wherever the user needs it and enables direct access to all key functions of the CASAMBI®lighting control system.  For instance the dimming, switching on and off of luminaires and also setting the RGB and RGBW in the colour selection field. The timer can also be used to preset various scenes.

Electrical data:

DC Ready: Yes

Acceptance tests:

Protection class: III

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 72,6 mm

Width (B): 30 mm

Height (H): 18 mm

Manufacturer: RP-Technik GmbH